***Section VII. Technical Specifications***

**Technical Specifications**

| **Specification** | **Statement of Compliance** |
| --- | --- |
| **STATE THE COMPLETE TECHNICAL SPECIFICATIONS** | *[Bidders must state here either “Comply” or “Not Comply” against each of the individual parameters of each Specification stating the corresponding performance parameter of the equipment offered. Statements of “Comply” or “Not Comply” must be supported by evidence in a Bidders Bid and cross-referenced to that evidence. Evidence shall be in the form of manufacturer’s un-amended sales literature, unconditional statements of specification and compliance issued by the manufacturer, samples, independent test data etc., as appropriate. A statement that is not supported by evidence or is subsequently found to be contradicted by the evidence presented will render the Bid under evaluation liable for rejection. A statement either in the Bidder's statement of compliance or the supporting evidence that is found to be false either during Bid evaluation, post-qualification or the execution of the Contract may be regarded as fraudulent and render the Bidder or supplier liable for prosecution subject to the applicable laws and issuances.]* |

**SUPPLY AND DELIVERY OF FURNITURE AND FABRICATION OF CUSTOMIZED EXHIBITION/ INTERIOR FIT-OUT AND FURNISHINGS BASED ON**

**THE PROVIDED CONCEPT**

**PHILIPPINES @ EXPO 2020 DUBAI**

**TECHNICAL SPECIFICATIONS**

**INSTRUCTIONS TO THE BIDDER:** Indicate **“COMPLY”** per line number under **Bidder’s Statement of Compliance** if Bidder can meet the technical specifications and project requirements. DO NOT LEAVE ANY BLANK. A **“YES”** or **“NO”** **ENTRY WILL NOT BE ACCEPTED. FAILURE TO CONFORM WILL RESULT IN A RATING OF “FAILED”.**

|  |  |  |
| --- | --- | --- |
| # | **MINIMUM SPECIFICATIONS** | **STATEMENT OF COMPLIANCE** |
| 1. | **Background of the Item/s being procured** |  |
| a. | Relative to the aforesaid event, DTI will need the services Supply and Delivery of Furniture and Fabrication of Customized Exhibition/ Interior Fit-out & Furnishings company who will customized based on the develop design of the Technical Consultant based on minimum requirements set by the Creative Team of the Philippines Pavilion in Expo 2020 Dubai. |  |
| 2. | **Purpose of the Procurement** |  |
| a. | The main objective of the proposal is to procure a services Supply and Delivery of Furniture and Fabrication of Customized Exhibition/ Interior Fit-out & Furnishings company who will customized based on the develop design of the Technical Consultant based on minimum requirements set. |  |
| b. | Supply and Delivery of Furniture and Fabrication of Customized Exhibition/ Interior Fit-out & Furnishings based on the provided concept design: Bidder will have to recommend the most available and cost-effective furniture items approximating the designs for the area given; |  |
| 3. | **Minimum Technical Specifications** |  |
| a. | **Area 6: Store and Travel Lounge (Golokal and Marahuyo** |  |
| i. | **Pedestal (Design 1)** |  |
| 1. | Quantity: 1 pc |  |
| 2. | Dimensions:Diameter: 0.50 MHeight: 1.00 M |  |
| 3. | Materials:12mm thk vanilla onyx solid surface table top on 3/4" thick marine plywood backing with 6mm thk champagne trim; champagne stainless steel mirror finish base |  |
| ii. | **Pedestal (Design 2)** |  |
| 1. | Quantity: 1 pc |  |
| 2. | Dimensions:Diameter: 0.50 MHeight: 0.80 M |  |
| 3. | Materials:12mm thk vanilla onyx solid surface table top on 3/4" thick marine plywood backing with 6mm thk champagne trim; champagne stainless steel mirror finish base |  |
| iii. | **Gondola** |  |
| 1. | Quantity: 4 pcs |  |
| 2. | Dimensions:Length: 1.50 MWidth: 0.60 MHeight: 1.65 M |  |
| 3. | Materials:10mm thk clear tempered glass adjustable shelves with 20mm thk champagne frames on 30mm x 30mm tubular steel support in champagne stainless steel finish; base and drawer in 3/4" thk marine plywood carcass with reflective high pressure laminate and concealed |  |
| iv. | **Glass Display Shelves** |  |
| 1. | Quantity: 9 pcs |  |
| 2. | Dimensions:Length: 0.90 MWidth: 0.60 MHeight: 1.20 M |  |
| 3. | Materials:10mm thk tempered glass adjustable shelves with 20mm thk champagne frames; 30mm x 30mm tubular steel supports in champagne mirror finish; base and drawer in 3/4" thk marine plywood carcass with reflective high pressure laminate finish and concealed |  |
| v. | **Hanger Rack** |  |
| 1. | Quantity: 2 pcs |  |
| 2. | Dimensions:Diameter: 0.60 MHeight: 1.55 M |  |
| 3. | Materials:Clothes rack in champagne stainless steel mirror finish with 12mm thick vanilla onyx solid surface on 3/4" thk marine plywood |  |
| vi. | **3 Tier Shelves** |  |
| 1. | Quantity: 9 sets |  |
| 2. | Dimensions:Length: 0.96 MWidth: 0.60 MHeight: 3.64 M |  |
| 3. | Materials:30mm x 30mm champagne powder coated tubular supports and frames; first tier in 12mm thk tempered glass; second and third tiers in matte black powder coated steel plate |  |
| vii. | **Wall Unit** |  |
| 1. | Quantity: 1 set |  |
| 2. | Dimensions:Length: 4.975 MDepth: 0.60MHeight: 2.40 M |  |
| 3. | Materials:Wall unit shelf with adjustable glass shelves of 10mm thk tempered glass and adjustable clothing rack on 20mm x 20mm tubular steel in champagne mirror finish; base storage shelves and shelf top of 3/4" MDF board in approved concrete look laminate |  |
| viii. | **Podium** |  |
| 1. | Quantity: 1 set |  |
| 2. | Dimensions:Length: 0.60 MWidth: 0.80 MHeight: 0.95 M |  |
| 3. | Materials:Base and cabinet in 3/4"thk marine plywood carcass with reflective high pressure laminate fin. |  |
| ix. | **Cashier Counter** |  |
| 1. | Quantity: 1 set |  |
| 2. | Dimensions:Length: 2.80 MWidth: 0.86 MHeight: 1.10 M |  |
| 3. | Materials:Counter table with top part in carrara marble with gold veins and base in white solid surface and champagne trims |  |
| x. | **Cashier Stool** |  |
| 1. | Quantity: 2 pcs |  |
| 2. | Dimensions:Length: 0.40 MWidth: 0.40 MHeight: 0.75 M (adjustable seat height) |  |
| 3. | Materials:Cashier stool in teal polyester upholstery; gas lift mechanism adjustable matte black aluminum legs; rounded flat base |  |
| xi. | **Storage Shelf** |  |
| 1. | Quantity: 5 sets |  |
| 2. | Dimensions:Length: 1.00 MWidth: 0.45 MHeight: 2.40 M |  |
| 3. | Materials:Storage shelf in 3/4" light grey lacquer finished marine plywood on 50mm x 50mm adjustable shelving brackets and frame support in lightgrey powder coat |  |
| xii. | **Wall Mounted Drop leaf table / Folding - Storage Room** |  |
| 1. | Quantity: 1 pc |  |
| 2. | Dimensions:Diameter: 0.60 MHeight: 0.75 M |  |
| 3. | Materials:Top and Base in charcoal powder coated aluminum |  |
| 4. | Color/style of top surface: Wood grains;supplier to provide swatches for approval |  |
| 5. | Wall mounted drop leaf table mechanism |  |
| xiii. | **Storage Room Stool** |  |
| 1. | Quantity: 2 pcs |  |
| 2. | Dimensions:Length: 0.50 MWidth: 0.46 MHeight: 0.76 M |  |
| 3. | Materials:Chair frame and seat in white reinforced polypropylene |  |
| xiv. | **Track Light** |  |
| 1. | Quantity: 1 set |  |
| 2. | Dimensions:Length: 10.15 MWidth: 4.85 M |  |
| 3. | Materials:Matte Black Powder coated finish |  |
| xv. | **Mirror** |  |
| 1. | Quantity: 1 pc |  |
| 2. | Dimensions:Width: 0.60 MHeight: 2.70 M |  |
| 3. | Materials:6mm thick mirror on 6mm thk marine plywood backing with champagne stainless steel frame |  |
| xvi. | **Velvet Curtain with S curve mechanism** |  |
| 1. | Quantity: 1 pc |  |
| 2. | Dimensions:Width: 2.50 MHeight: 5.30 M |  |
| 3. | Materials:Velvet drapes in putty color; S-curve recessed housing |  |
| b. | **Area 8: Mangrove Cafe** |  |
| i. | **Back Counter** |  |
| 1. | Quantity: 1 setSet includes: 3 different counters |  |
| 2. | Dimensions:Counter 1Length: 1.00 MDepth: 0.65 MHeight: 0.80 MCounter 2Length: 1.00 MDepth: 0.65 MHeight: 0.80 MCounter 3Length: 1.00 MDepth: 0.65 MHeight: 0.80 M |  |
| 3. | Materials:Counter 1 & 23/4” thk Marine Plywood Carcass in Black High-Pressure Laminate Finish20 mm thk Raven Onyx Solid Surface countertopCounter 33/4” thk Marine Plywood Carcass in Black High-Pressure Laminate Finish20 mm thk Raven Onyx Solid Surface countertop6 mm thk Clear Double-Glazed glass case w/ shelves |  |
| ii. | **Café Counter** |  |
| 1. | Quantity: 1 set |  |
| 2. | Dimensions:Length: 3.52 MWidth: 4.12 MCountertop Height: verify on drawingsOverall Height: 1.40 M |  |
| 3. | Materials:3/4” thk Marine Plywood Carcass in Black High-Pressure Laminate Finish |  |
| 4. | 20 mm thk Raven Onyx Solid Surface countertop |  |
| 5. | Glass Display refrigeration built-in look |  |
| iii. | **Indoor Chair** |  |
| 1. | Quantity: 30 pcs |  |
| 2. | Dimensions:Depth: 0.45 MWidth: 0.52 MHeight: 0.85 M |  |
| 3. | Materials:Dinnig Chair w/ steel lattice work |  |
| 4. | Back frame & legs in charcoal grey painted finish |  |
| 5. | Upholstery in grey polyester fabric |  |
| iv. | **6-Seater Table** |  |
| 1. | Quantity: 2 sets |  |
| 2. | Dimensions:Length: 1.90 MWidth: 1.00 MTable Height: 0.75 MOverall Height: 1.75 M |  |
| 3. | Materials:Partition: 5mm thk clear acrylic |  |
| 4. | Table top: 20mm thk MDF board in grey laminate finish |  |
| 5. | Support: 1”x1” tubular steel in bronze painted finish |  |
| v. | **4-Seater Table** |  |
| 1. | Quantity: 3 sets |  |
| 2. | Dimensions:Table Diameter: 1.00 MTable Height: 0.75 MOverall Height: 1.75 M |  |
| 3. | Materials:Partition: 5mm thk clear acrylic |  |
| 4. | Table Top: 20mm thk MDF board in grey laminated finish |  |
| 5. | Support: 1”x1” tubular steel in bronze painted finish |  |
| vi. | **2-Seater Table** |  |
| 1. | Quantity: 3 sets |  |
| 2. | Dimensions:Table Diameter: 0.90 MTable Height: 0.75 MOverall Height: 1.75 M |  |
| 3. | Materials:Partition: 5mm thk clear acrylic |  |
| 4. | Table top: 20mm thk MDF board in grey laminate finish |  |
| 5. | Support: steel in bronze painted finish |  |
| vii. | **Outdoor Chair** |  |
| 1. | Quantity: 28 pcs |  |
| 2. | Dimensions:Length: 0.58 MDepth: 0.55 MHeight: 0.75 M |  |
| 3. | Materials:Dining Chair with steel lattice work  |  |
| 4. | back rest and frame wrapped in charcoal grey  |  |
| 5. | twisted cotton fabric & steel legs in gray painted fin. |  |
| viii. | **4-Seater Table (outdoor)** |  |
| 1. | Quantity: 7 sets |  |
| 2. | Dimensions:Table Diameter: 1.00 MFrame Diameter: 2.50 MTable Height: 0.75 MOverall Height: 2.50 M |  |
| 3. | Materials:Roof: 6mm thk polycarbonate |  |
| 4. | Partition: 5mm thk clear acrylic |  |
| 5. | Table top: 20mm thk grey solid surface |  |
| 6. | Support and Frames: 2”x2” tubular steel in bronze painted finish and flat steel in bronze painted finish |  |
| C. | **Area 9: Executive Offices** |  |
| i. | **Reception Counter** |  |
| 1. | Quantity: 1 set |  |
| 2. | Dimensions:Length: 3.00 MDepth: 0.45 MHeight: 1.10 M |  |
| 3. | Materials:Base part in dark gray high gloss lacquer finish metal and upper part in loam solid surface |  |
| ii. | **Reception Staff Chair** |  |
| 1. | Quantity: 2 sets |  |
| 2. | Dimensions:Width: 0.625 MDepth: 0.56 MHeight: 0.82 M(adjustable seat height) |  |
| 3. | Materials:Lowback chair with arm rest upholstered in grey polyester fabric with polypropylene legs in matte black  |  |
| iii. | **Waiting Area Couch** |  |
| 1. | Quantity: 1 pc |  |
| 2. | Dimensions:Length: 2.40 MDepth: 0.85 MHeight: 0.85 M |  |
| 3. | Materials:Backrest frame wrapped in charcoal grey cotton fabric upholstery in olive green linen fabric base in tanguile wood matte finish |  |
| iv. | **VIP Side Table** |  |
| 1. | Quantity: 1 pc |  |
| 2. | Dimensions:Diameter: 0.55 MHeight: 0.60 M |  |
| 3. | Materials:3/4” thk tubular bar steel pipe in powder coat finish with 3/4” thk calacata light grey marble top |  |
| v. | **Conference Chair** |  |
| 1. | Quantity: 12 pc |  |
| 2. | Dimensions:Width: 0.63 MDepth: 0.68 MHeight: 0.95 M(adjustable seat height) |  |
| 3. | Materials:Base in stainless steel chrome finish with upholstery in blue gray polyester fabric |  |
| vi. | **Conference Table** |  |
| 1. | Quantity: 1 pc |  |
| 2. | Dimensions:Length: 3.50 MDepth: 1.60 MHeight: 0.75 M |  |
| 3. | Materials:12mm thk clear gray tempered glass with legs of 80-100mm diameter hammered stainless stee**l** |  |
| 4. | It should fit all entry point (doors and stair going up to Executive offices) going the conference room |  |
| vii. | **VIP Visitors Chair** |  |
| 1. | Quantity: 2 pc |  |
| 2. | Dimensions:Width: 0.45 MDepth: 0.50 MHeight: 0.85 M |  |
| 3. | Materials:High back chair with low arm rest and 4 narrow wooden legs stained in macassar ebony:Polyester Fabric in blush |  |
| viii. | **VIP Office Desk** |  |
| 1. | Quantity: 1 pc |  |
| 2. | Dimensions:Length: 2.00 MDepth: 0.80 MHeight: 0.75 M |  |
| 3. | Materials:12mm thk clear gray tempered glass with 30x150mm brushed stainless steel legs |  |
| ix. | **VIP Ergonomics Chair** |  |
| 1. | Quantity: 1 pc |  |
| 2. | Dimensions:Width: 0.80 MDepth: 0.79 MHeight: 0.82 M(adjustable seat height) |  |
| 3. | Materials: |  |
| 4. | High Back in teal polyester fabric |  |
| 5. | Stainless steel Starbase with stainless Casters |  |
| 6. | with adjustable gaslift |  |
| 7. | 360 degrees swivel function |  |
| 8. | Ergonomic, dynamic and durable |  |
| x. | **Staff Work Station Cluster for 4**  |  |
| 1. | Quantity: 1 set |  |
| 2. | Dimensions:Length: 2.40 MWidth: 1.20 MHeight: 0.80 M |  |
| 3. | Materials:¾ marine plyboard carcass with white high pressure laminate soft-close drawers and keyboard drawers in natural walnut high pressure laminate |  |
| 4. | tuckable and easy to removefabric desk dividers; Supplier to providefabric swatches for approval |  |
| 5. | with modesty panels (as necessary) |  |
| 6. | Grommets provided for electrical andcommunications wire management |  |
| 7. | Electrical and communication systemintegration available |  |
| 8. | With electrical/power sockets, Ethernetcable, USB hub on top of the table,depressed of at least 5-6 inches |  |
| 9. | with side drawers for each staff (4 sets) |  |
| 10. | with drawer tray divider |  |
| 11. | drawer folder divider |  |
| 12. | Central locking system |  |
| xi. | **Staff Work Station Cluster for 2** |  |
| 1. | Quantity: 1 set |  |
| 2. | Dimensions:Length: 1.20 MWidth: 1.20 MHeight: 0.80 M |  |
| 3. | Materials:3/4" thk marine plywood carcass with white high-pressure laminate soft-close drawers and keyboard drawer in natural walnut high-pressure laminate |  |
| 4. | tuckable and easy to removefabric desk dividers; Supplier to providefabric swatches for approval |  |
| 5. | with modesty panels (as necessary) |  |
| 6. | Grommets provided for electrical andcommunications wire management |  |
| 7. | Electrical and communication systemintegration available |  |
| 8. | With electrical/power sockets, Ethernetcable, USB hub on top of the table,depressed of at least 5-6 inches |  |
| 9. | with drawer pencil tray divider |  |
| 10. | drawer folder divider |  |
| 11. | Central locking system |  |
| xii. | **Staff Ergonomics Chair** |  |
| 1. | Quantity: 6 pcs |  |
| 2. | Dimensions:Length: 0.64 MWidth: 0.60 MHeight: 0.88 M(adjustable seat height) |  |
| 3. | Materials:Ergonomic swivel office chair in dark gray mesh fabric upholster |  |
| 4. | Midback design |  |
| 5. | with armrest support and legs in matte black polypropylene |  |
| 6. | with adjustable gaslift mechanism |  |
| 7. | Dark Gray mesh fabric upholstery back & seat |  |
| 8. | Backrest support in matte gray polypropylene |  |
| 9. | Star base with 5 matte black nylon casters |  |
| 10. | Supplier to provide Colors/Fabricdesign swatches for approval |  |
| 11. | 360 degrees swivel function |  |
| xiii. | **Kitchen Cabinet 1** |  |
| 1. | Quantity: 1 set |  |
| 2. | Dimensions:Length: 1.84 MDepth: 0.65 MHeight: 2.20 M |  |
| 3. | Materials:3/4” thk marine plywood with charcoal high-pressure laminate finish carcass |  |
| 4. | 20mm thk witch hazel solid surface countertop with cooktop |  |
| 5. | Door soft closing mechanism and with cabinet door damper |  |
| xiv. | **Kitchen Cabinet 2** |  |
| 1. | Quantity: 1 set |  |
| 2. | Dimensions:Length: 3.20 MDepth: 0.60 MHeight: 2.20 M |  |
| 3. | Materials:3/4” thk marine plywood with charcoal high-pressure laminate finish carcass |  |
| 4. | 20mm thk witch hazel solid surface countertop with cooktop |  |
| 5. | Door soft closing mechanism and with cabinet door damper |  |
| xv. | **VIP Lavatory Counter with Mirror** |  |
| 1. | Quantity: 1 set |  |
| 2. | Dimensions:Length: 3.26 MDepth: 1.325 MHeight: 2.850 M |  |
| 3. | Materials:3/4" thk marine plywood carcass in matte charcoal lacquer finish with 10mm thk vanilla onyx solid surface on 3/4” thk marine plywood backing |  |
| 4. | 5mm thk clear mirror with 20mm thk charcoal grey trim |  |
| xvi. | **Office Lavatory Counter with Mirror** |  |
| 1. | Quantity: 1 set |  |
| 2. | Dimensions:Lavatory Counter: 0.80 M x 0.60 M x 0.10 M (LxWxH)Mirror: 3.00 M x 2.00 M x 5mm (WxHxThk) |  |
| 3. | Materials:Lavatory Counter: 10mm thk vanilla onyx solid surface on 3/4” Marine Plywood backing with 20mm thk charcoal grey trim |  |
| 4. | 5mm thk clear mirror |  |
| xvii. | **Window Roller Shades System** |  |
| 1. | Quantity: 1 set |  |
| 2. | Dimensions:Linear meterReception: 4.01 MConference Room: 12.86 MIT Room: 1.63 MVIP office/ Comm. Gen. Office: 4.64 MStaff office: 8.23 MTotal linear meter: 31.37 M |  |
| 3. | Materials:Blackout roll ups |  |
| 4. | Crème linen fabric |  |
| 5. | Metal/plastic beaded cord |  |
| 6. | Fabric material: provide swatch or sample forapproval |  |
| 7. | Soil and dust resistant |  |
| 8. | Good Sound absorption |  |
| D. | **PH PAVILION – WASTE BIN REQUIREMENTS** |  |
| i. | **Outdoor Waste Bin Requirements** |  |
| 1. | Quantity: Ground Floor: 4 setsSecond Floor: 3 setsRoof Deck: 3 Sets(See reference plan for the exact location) |  |
| 2. | Dimensions:Length: 0.40MWidth: 0.40 MHeight: 0.80 M |  |
| 3. | Material:Painted Metal |  |
| 4. | Set includes 3 Types of Bins:General WasteOrganic WasteRecyclable(see reference drawing) |  |
| ii. | **Indoor Waste Bin Requirements** |  |
| 1. | Quantity: Executive Offices: 12 setsBoutique: 2 setsMangrove Cafe: 2 Sets(See reference plan for the exact location) |  |
| 2. | Dimensions:Length: 0.25MWidth: 0.25 MHeight: 0.35 M |  |
| 3. | Material:Stainless Steel |  |
| 4. | **Duration of the Contract** |  |
| a. | The winning bidder shall provide partial delivery on readily available items on November – December 2020 |  |
| b. | The winning bidder shall complete the fabrication, delivery and installation of work within July 2021 |  |
| 5. | **Warranty** |  |
| a. | Replacement of defective fixtures/ furniture/ equipment/ appliance and materials to be used for repairs and repainting jobs within the duration of the warranty (Warranty period will run until March 2022 and/or last day of the EXPO Event duration) |  |
| b. | The bidder further warrants that all Goods supplied under this Contract shall have no defect, arising from design, materials, or workmanship or from any act or omission of the Supplier that may develop under normal use of the supplied Goods in the conditions prevailing in the country of final destination |  |
| c. | Bidder shall be responsible for all the cost related to the warranty period (Warranty period will run until March 2022 and/or last day of the EXPO Event duration). |  |
| d. | Warranty from delivery date to end of event duration as scheduled by the EXPO organizer |  |
| e. | Supplier should provide spare parts as needed within the warranty period. |  |
| 6. | **Other Requirements** |  |
| a. | During the post qualification, the winning bidder isrequired to submit: |  |
| b. | actual materials to use including specifications |  |
| c. | actual fabric swatches for approval |  |
| d. | actual wood stain swatches for approval |  |
| e. | Must provide photo or brochure and technicalspecifications of actual items to be delivered |  |
| f. | Contractor must provide an as-built drawings/diagrams/layout/shop drawing of the fixtures, furniture, furnishing and equipment/appliances that will be supplied, delivered, installed in the Philippines Pavilion in hard and e-copy and/or as needed by the organizer |  |
| g. | Documentation of financial breakdown/cost for items (in unit prices and total prices) including assemble/ installation, repainting/ repair and warranty services and others. |  |
| h. | This Contract shall be interpreted in accordance with the laws of the Republic of the Philippines. |  |
| i. | This Contract has been executed in the English language, which shall be the binding and controlling language for all matters relating to the meaning or interpretation of this Contract. All correspondence and other documents pertaining to this Contract exchanged by the parties shall be written in English |  |
| 7. | **Payment Terms** |  |
| a. | Payment shall be made upon issuance of Certificate of Final Acceptance from the head of the Procuring entity (Alternate Commissioner General) |  |
| b. | Posting of 5% special bank guarantee(as warranty for defects)Submission of 5% special bank guarantee upon signing of contract of the winning bidder and approval of Notice to Proceed |  |
| c. | 1ST PARTIAL DELIVERYwithin 2020Processing of payment upon submission of accomplishment report and list of items initially delivered on site and ensure that the 5% bank guarantee is already submitted |  |
| d. | 2nd (FULL) DELIVERY and HAND-OVERin 2021 but not later than July 2021Processing of payment upon full delivery of the items, no later than July 2021; upon submission of the Accomplishment report and 100% complete and show ready and final acceptance/ certifications from the head of the Procuring entity (Alternate Commissioner General)(Monthly progress report should be submitted every 20th day of the month) |  |
| e. | Release of 5% special bank guaranteeShall be release to winning bidder/ supplier in April 2022 after the EXPO. |  |
| 8. | **Timeliness for Implementation of the Project** |  |
| a. | 1st Partial Delivery within November – December 2020 or as stated in the Terms of Reference |  |
| b. | Customized and Assembly PhaseDuration: November 2020 – 30 June 2021 |  |
| c. | Delivery and Installation PhaseDuration: 1-25 July 2021 |  |
| d. | 2nd (Full) Delivery and Hand-overDuration: 26 – 31 July 2021 |  |

**I hereby certify that the statement of compliance to the foregoing technical specifications are true and correct, otherwise, if found to be false either during bid evaluation or post-qualifications, the same shall give rise to automatic disqualification of our bid.**

|  |  |
| --- | --- |
| Name of Company: |  |
|  |  |
|  |  |
| Signature: |  |
|  | Signature Over Printed Name of Authorized Representative |
| Date: |  |

Conforme:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name & Signature of Authorized Representative

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date signed